Title: CFMEUVT 34682 plant_checklist_1.indd

dAte: / / 

Pre-Start Inspection Checklist 

If any item below is not ticked, the concrete must not be unloaded or emptied until the issue has been resolved. 
Documentation Checklist 

2) Logbook 

4) Risk assessment/Hazard checklist 

6) Driver inducted into Concrete Company’s SWMSs 

8) Documented proof of ‘cleaning/de-dagging’ agitator for each truck (maximum 3-monthly cycle) 

10) Driver has Heavy Rigid Licence 

Visual Inspection Checklist 

2) Reverse beepers/warning signals working 

4) Fire extinguisher fitted anf fully operational 

6) All controls clearly labelled, marked and operating, including lights, horn, brakes etc 

8) Truck does not sag to one side (check for flat tyres, overloading or incorrect loading) 

10) No cracks in lights 

continued overleaf 

At completion of plant inspection, confirm that the operator has completed their daily pre-start checks and entered this in their logbook. 
www.cfmeuvic.com.au 

Wheels and rims undamaged (A bent or damaged rim might cause a tyre to lose pressure or come off the 
14) 
rim. Multi-piece rims are under high pressure, and can explode if damaged.) 

16) Tyres properly fitted, and tread niether damaged nor worn (Worn front tyres = potential loss of steering. ) 

18) Truck has fall protection for both climbing agitator ladder and standing on agitator platform 

20) Driver wearing high vis-clothing/fluro safety vest 

site nAMe: |
Address: |

At completion of plant inspection, confirm that the operator has completed their daily pre-start checks and entered this in their logbook. 
www.cfmeuvic.com.au