

**SUMMARY**

[Golden Rule 1 - Working at height 4](#_TOC_250007)

[Golden Rule 2 - Energized systems 6](#_TOC_250006)

[Golden Rule 3 - Fire safety 8](#_TOC_250005)

[® Golden Rule 4 - Toxic gases 10](#_TOC_250004)

[Golden Rule 5 - Lifting operation 12](#_TOC_250003)

[Golden Rule 6 - Confined space 14](#_TOC_250002)

[Golden Rule 7 - Management of change 16](#_TOC_250001)

-i Golden Rule 8 - Driving safety 18

i- Golden Rule 9 - Permit to work 20

[Golden Rule 10 - Excavation safety 22](#_TOC_250000)



With the **Stop Work Authority,** anyone working within Eni sites, as either an employee or contractor, is empowered to interrupt an activity whenever he observes an unsafe act

or an unsafe condition.

We cannot accept to have an injury due to a predictable cause, or to actions that are unsafe.

Therefore, whenever we find a hazard, we have to report it in order to eliminate it.

It is our duty to ensure that any activity is conducted in a safe manner, keeping both ourselves and our colleagues safe!

**You have the**

**stop work authority!**

**Safety is our value**

This booklet provides a concise guide to the basic rules

to be followed during working activities, with the intention

to raise awareness on safety at site respecting the Eni minimum Safety requirements.

The **10 Safety Golden Rules** must become part of our way of approaching and conducting any working activity.

## We must ensure that

* All job activities are adequately planned, assessed and executed.
* All personnel are adequately informed, trained and have all the

necessary equipment to perform the work.

* All personnel are empowered to intervene and to stop activities anywhere or at any time when the Safety Golden Rules are

not correctly applied.

## Our commitment

The 10 Safety Golden Rules apply to anyone working within Eni sites, as either an employee or contractor, anywhere in the world.

#### Introduction

**Top and Middle Management**

* Provide adequate resources to support the continued

implementation of the 10 Safety Golden Rules.

* Demonstrate their personal commitment, leadership and accountability.

#### Supervisors

* Ensure that work conditions are safe.
* Ensure, leading by example, that their teams know

and observe the rules and that they comply with them before

starting, during and at the end of a working activity.

#### Workers

* Be responsible for the safety of themselves and that of their co-workers.
* Be aware that compliance is mandatory.
* Immediately report to their supervisor/person in charge, about

any unsafe event (i.e. accident, near miss, unsafe act, unsafe

condition) that occurs at the work site.

# Golden Rule 1 – Working at height



**Controls and monitoring of the reliability of equipment and protection systems during work at height activities ensure the workers safety.**

#### Golden Rule 1 – Working at height

**PLAN**

* Avoid working at height wherever a practical alternative option is available.
* Prefer fall prevention systems to fall protection systems.
* Guarantee that fall protection systems (e.g., full body safety

harness, shock absorbing lanyards) are periodically inspected

and maintained by a competent person.

* Guarantee that arrangements for emergency rescue at height are in place.

**READY?**

* Is the PTW in place, completed with the risk assessment for each work at height activity?
* Are scaffolds inspected by a competent person prior to use

and equipped with a valid tag/panel certifying the inspection?

* Are personnel working at height provided with specific training?
* Are the PPEs identified by the Employer in the specific risk

assessment for the required task, in good condition and worn

by all people?

### GO!

* Guarantee that work surfaces and holes are always adequately protected from fall of personnel and objects.
* Guarantee that all scaffolds are built according to the vendor

manual/specifications or a specific project done by an

authorized engineer.

* Guarantee that only authorized workers (specifically trained) access the scaffolds.

# Golden Rule 2 – Energized systems

**Implementation of procedures, controls and specialized personnel guarantee safety during activities where energized systems are present.**

#### Golden Rule 2 – Energized systems

**PLAN**

* Verify that a specific energy isolation procedure is in place.
* Each job shall be both risk assessed and performed

by competent personnel.

* Ensure that the permit to work refers unambiguously

to the equipment on which the intervention is requested.

* Guarantee to periodically inspect and maintain portable appliances and equipment, which work under energy.

**READY?**

* Is an energy isolation certificate completed in conjunction with and referred to in the PTW?
* Have you verified that no stored energy or other hazards

remain prior to start your job, and that the energy isolation

is properly done?

* Does authorized competent personnel, who has been appointed by the Company Management, perform

the energy isolation?

* Are the PPEs identified by the Employer in the specific risk assessment for the required task, in good condition and worn

by all people?

### GO!

* Do not carry out unauthorized activities. Follow the provisions of the permit to work.
* Use lockout and tagout devices to inform of isolation and to

prevent non-authorized operations.

* Ensure that no work or equipment movement is allowed under or near an overhead power line unless precautions

have been taken.

# Golden Rule 3 – Fire safety

**Fire risk must be assessed and control measures such as procedures and active/passive fire protection systems implemented.**

#### Golden Rule 3 – Fire safety

**PLAN**

* Ensure that a competent person for each site performs a fire risk assessment.
* Guarantee that a fire emergency response plan is developed

and all personnel is trained.

* Guarantee the use of a specific PTW when the activity foreseen the use of free flame, equipment with ignition

sources, and foresee the proper fire fighting measures.

* Plan, for a sufficient number of workers, specific training in the proper use of firefighting equipment.
* Periodically inspect and maintain the fire prevention and

protection measures.

**READY?**

* Are all work places equipped with means of fire detection, alarm and firefighting equipment?
* Are sources of ignition under control and unnecessary ones

removed?

* Are escape routes and muster points clearly marked and kept easily accessible at all time?

### GO!

* Handle and store flammable materials properly.
* Ensure that workers do not smoke at the plant, except

in authorized areas, and they do not use naked flames a/o

non-explosion proof equipment unless expressly authorized.

* Keep all areas clean and tidy.

# Golden Rule 4 – Toxic gases



**Procedures, staff training, specific collective and personal protective equipment are required to work**

**in the presence of toxic gases.**

#### Golden Rule 4 – Toxic gases

**PLAN**

* Guarantee that the operating procedures, work instructions and ERP have been developed considering the risks related

to toxic gas release.

* Guarantee that everybody is informed on toxic gas risk

and properly trained on their specific role during emergencies,

and on collective/personal protective equipment.

* Guarantee that each worker has both a personal toxic gas detector and a proper breathing escaping device (full face

mask / hood with specific filter / air bottle).

* Post safety signs and any other means, warning of the potential presence of toxic gas.

**READY?**

* Are you authorized to enter a toxic gas classified area?
* Is the ERT present on site and alerted?

### GO!

* Always wear your full face mask / hood with specific

filter / air bottle, to be used exclusively in case of emergency,

and your personal detection devices when working in an area where there is or could be the presence of toxic gas (provided that breathable air is guaranteed, otherwise, use a breathing apparatus).

# Golden Rule 5 – Lifting operation



**Lifting operations properly planned, implemented and monitored, prevent the workers risk of falling or being**

**crushed or struck.**

#### Golden Rule 5 – Lifting operation

**PLAN**

* Plan the lift with a specific risk assessment.
* Always inspect the equipment/machines and accessories as per

manufacturer’s instructions and site procedure requirement:

check and record damages, color code, SWL and certificate.

* Lifting authority be involved in all activities.
* Personnel lifts shall be done only with man-rated equipment

and under a PTW.

**READY?**

* Is lifting equipment certified by a Third Party in accordance with relevant local legislation or international standards and regularly

maintained according to the planned schedule?

* Are all persons engaged in lifting and hoisting operations competent for that role and supervised at all times?
* Are lifting and hoisting equipment, machines and accessories

(cranes, forklifts, slings, handles, hooks, baskets, etc.) in good

condition according to national legislation and international best practices?

* Have you verified that the lifting area is marked out

to prohibit unauthorized access?

* Are the PPEs identified by the Employer in the specific risk assessment for the required task, in good condition and worn

by all people?

### GO!

* Always ensure the presence of a banksman during the entire lifting operation and avoid unplanned blind lifts.
* Never allow personnel to be under or close to suspended

loads for any reason.

* Ensure that the lifting operator keeps the machine/equipment under control at all time.

# Golden Rule 6 – Confined space



**Atmospheric testing, specific training on confined space activities,**

**implementation of dedicated emergency procedures, are mandatory to work safely in a confined space.**

#### Golden Rule 6 – Confined space

**PLAN**

* Each job shall be risk assessed and all hazards and controls shall be identified and implemented.
* Plan specific training for all persons engaged in confined

spaces activities.

**READY?**

* Is a Confined Space certificate completed in conjunction with and referred to in the PTW?
* Did you verify that the confined space is positively isolated

from all possible sources of hazards?

* Have qualified and authorized personnel tested and recorded the atmosphere inside the confined space as designated

in the permit/confined space entry certificate?

* Is the Emergency Response and Rescue Plan prepared

and tested? Is the ERT ready in location and communication

means ready and tested?

* Are the PPEs identified by the Employer in the specific risk assessment for the required task, in good condition and worn

by all people?

### GO!

* Suspend the work if ERT and/or means of communications are unavailable on site.
* Suspend the work if a dedicated qualified attendant (watcher)

is not present close to the confined space.

* Suspend the work if there is no specific PTW and Confined space certificate for the activity.
* Suspend the work if Rescue Equipment are not in place.
* Keep always visual or voice contact with the entrants.

# Golden Rule 7 – Management of change



**Any plant/organizational change must be identified, assessed and authorized by the responsible of the work place.**

#### Golden Rule 7 – Management of change

**PLAN**

* Identify, analyze and assess any change or deviation to plant design, work procedures/practices and organization.
* Support any change, in particular overriding/disabling/change

of a safety critical element, with a specific risk assessment.

**READY?**

* Is the change, in particular deviations from mandatory requirements, duly structured, documented and approved by

a Company authorized and competent person?

* Is the change properly recorded and tracked in a dedicated system?

### GO!

* Communicate any change to all concerned personnel and keep track of the identified and implemented actions.

# Golden Rule 8 – Driving safety



**Driving behavior and recommendations for proper vehicle management reduce the risk of accidents.**

#### Golden Rule 8 – Driving safety

**PLAN**

* Always ensure that the driver is in good physical condition.
* Drivers shall be certified and authorized for driving the utilized

vehicle.

**READY?**

* Is your vehicle in good condition and regularly maintained?
* Are seat belts fastened and appropriate shoes worn?
* Are you free from the influence of alcohol and drugs?
* Are loads properly secured and within the capacity

of the vehicle?

* Are you sufficiently rested to drive a vehicle?

### GO!

* Adopt defensive behavior in respect of other road users.
* Respect speed limits, adjusting your speed according to road

and weather conditions, local legislation and Company rules.

* When you drive, do not use any mobile phone and respect the daily maximum driving hours and rest period.

# Golden Rule 9 – Permit to work



**Work permit is an essential and mandatory management tool to be adopted for non-routine or dangerous activities.**

#### Golden Rule 9 – Permit to work

**PLAN**

* A PTW system must be in place with the relevant supporting procedures and systematically implemented.
* Simultaneous/concurrent activities shall be planned

and subjected to risk assessment and PTW in order

to eliminate/reduce interferential risks.

* Non-routine and high-risk activities shall be planned and subjected to risk assessment and PTW.
* Guarantee that all personnel receive proper training on using

the PTW system.

**READY?**

* Is the PTW discussed in dedicated meetings?
* Have all personnel working under a PTW received

the necessary information about its contents?

* Have you verified that all requirements specified in the PTW are implemented on site?

### GO!

* Suspend and re-assess your work if a change occurs in the scope of the work, tools, equipment, personnel, shift change

or any other condition of the PTW.

# Golden Rule 10 – Excavation safety

**Soil characterization, protected excavation areas and correct use of machinery, guarantee the workers safety.**

#### Golden Rule 10 – Excavation safety

**PLAN**

* A soil survey shall be carried out and all the risks shall be identified and assessed.
* Always consider underground services in the area, those shall

be identified, marked and isolated (if necessary).

* Plan specific training for all personnel involved in excavation works.

**READY?**

* Do you have a valid excavation clearance certificate and the PTW?
* Has the site been inspected by a competent person?
* Are the PPEs identified by the Employer in the specific risk

assessment for the required task, in good condition and worn

by all people?

### GO!

* Effectively shore, slope, bench, barricade and sign all excavations.
* Provide suitable entry and exit point when working in trenches,

considering any possible emergency and weather condition.

* Guarantee that workers stand outside the area of action of the excavator.

Printed in February 2018



