Operator/Inspector______________________________ Date_______________ Time______________ Serial Number_________________________ Machine Hours_________________________ 

What are you inspecting? 	9 	What are you looking for? 	9	 Evaluator Comments 	

For more information, please refer to the Operation and Maintenance Manual or any other applicable manuals and instructions for this product. If you have questions, please contact your local Caterpillar dealer. 
FROM THE GROUND 

Tires, Wheels, Stem Caps 		Inflation, Leaks, Damage, Wear 			
Duo-cone seal area 		Damage, Leaks 			
Underneath Machine 		Leaks, Damage 			
Differentials, Brakes, Transmission 		Leaks 			
Front Suspension Cylinders 		Leaks, Proper Cylinder Height 			
Engine Area 		Leaks, Damage, Belt / Hose Condition 			
Engine Oil (785/789/793/797) 		Fluid Level (Record Oil Additions if Equipped with Oil Renewal System) 			
Fuel Filters / Water Separator 		Leaks / Drain Water (if equipped) 			
Fuel Tank 		Mounting Brackets, Welds, Leaks, Drain Water and sediment 			
Hoist Cylinders 		Wear, Damage, Leaks 			
Dump Body and Truck Frame 		Damage, Wear, Distortion, Presence of Frame and Body Support Pads 			
Rear Tire Rock Ejectors 		Free Movement 			
Primary Air Tank (777/793/797) 		Drain Moisture 			
Steps & Handholds 		Condition & Cleanliness 			
Torque Converter Case (793/797) 		Transmission and Torque Converter Fluid Level, Damage, Leaks 			
Hoist, Converter, and Brake Oil Tank (777/785/789) 		Fluid Level, Damage, Leaks 			
Steering Oil Tank (797) 		Fluid Level, Damage, Leaks 			
Transmission Oil Tank (777/785/789) 		Fluid Level, Damage, Leaks 			
Steps, Handholds 		Condition and Cleanliness 			
Lights, Front and Rear 		Function, Damage to Lens, Housing, or Wiring 			
Radiator 		Debris between Radiator and Grill, Fin Blockage, Leaks 			
ROPS 		Damage, Loose Mounting Bolts 			

ENGINE COMPARTMENT (TOP PLATFORM) 

Engine Oil (777) 		Fluid Level (Record Oil Additions if Equipped with Oil Renewal System) 			
Engine Coolant 		Fluid Level (jacket water, aftercooler) 			
Radiator 		Fin Blockage, Leaks 			
All Hoses 		Cracks, Wear Spots, Leaks 			
All Belts 		Tension, Wear, Cracks 			
Overall Engine Compartment 		Trash or Dirt Buildup, Leaks 			

ON THE MACHINE, OUTSIDE THE CAB (TOP PLATFORM) 

Handholds 		Condition and Cleanliness 			
Mirrors 		Damage, Adjust for Best Visibility 			
ROPS 		Damage, Loose Mounting Bolts 			
Dump Body above Platform 		Damage, Wear, Distortion 			
Pre-Cleaner 		Debris 			
Air Filter 		Restriction Indicator, Dust Valves Unplugged 			
Steering Oil Tank (777/785/789/793) 		Fluid Level, Damage, Leaks 			
Fire Extinguisher 		Charge, Damage 			
Windshield, Windows 		Broken Glass, Cleanliness 			
Windshield Wipers / Washers 		Wear, Damage / Fluid Level 			
Doors 		Open properly, broken glass 			
Air Conditioner Filter 		Dirt, Dust 			
Primary Air Tank (785/789) 		Drain Moisture 			
Secondary Air Tank 		Drain 			
Battery Compartment 		Cleanliness, Loose Nuts & Bolts 			

INSIDE THE CAB 

Seat 		Adjustment, Able to Reach Pedals 			
Seat Belt & Mounting 		Damage, Wear, Adjustment, Age 			
Horn, Backup Alarm, Lights 		Proper Function 			
Mirrors 		Damage, Adjust for Best Visibility 			
Recirculation Cab Air Filter 		Dirt, Dust 			
Gauges, Indicators, Switches, Controls 		Damage, function 			
Overall Cab Interior 		Cleanliness 			

HTTP://SAFETY.CAT.COM/CHECKLISTS V0611.2 
CAT, CATERPILLAR, their respective logos, “Caterpillar Yellow” and the POWER EDGE trade dress, as well as corporate and product identity used herein, are trademarks of Caterpillar and may not be used without permission. © 2009 Caterpillar All Rights Reserved