What are you inspecting?		What are you looking for?		Evaluator Comments	
For more information, please refer to the Operation and Maintenance Manual or any other applicable manuals and instructions for this product. If you have questions, please contact your local Caterpillar dealer

DRIVER/PASSENGER SIDE	
External Side Mirrors (Right and Left)		Cracks, Broken, Working condition, Properly placed			
Tires		Properly inflated, Adequate tread			
Windows		Broken, Cracked, Missing, Cleanliness			
REAR OF VEHICLE	
Bumper		Loose, Missing, Damage 			
License Plate 		Current sticker, Cleanliness, Properly attached 			
Inside of trunk or truck bed 		Spare tire, Jack, Wrench, Free of debris, Cleanliness 			
Brake lights 		Tested and working properly, Broken 			
Rear Window 		Broken, Cracked, Missing, Cleanliness 			
FRONT OF VEHICLE	
Headlights (normal and bright) 		Tested and working properly, Broken 			
Turn Signals 		Tested and working properly, Broken 			
Bumper 		Securely attached 			
Windshield 		Broken, Cracked, Missing, Cleanliness 			
Windshield wiper blades 		Properly installed, Damaged, Broken, Proper working order 			
UNDER THE HOOD	
Battery 		Properly secured, Cables secured, Working properly 			
Air Filter 		Cleanliness 			
Leaks 		Cracks in hoses, Fluid on ground, Leaks from filters 			
Windshield Fluid 		Proper fluid level 			
Transmission Fluid 		Proper fluid level 			
Engine Coolant 		Proper coolant level 			
Engine Oil 		Proper oil level 			
INSIDE CAR	
Overall Interior 		Cleanliness & free of debris 			
Parking Brake 		Tested on grade and working properly 			
Horn 		Tested and working properly 			
Seat Belts 		Tested and working properly, Frays, Cuts, Tears, Snags, Roping 			
Gauges 		Working condition 			
Rearview Mirror 		Properly placed, Working condition, Cleanliness 			
IF REQUIRED	
Wheel Chocks 		Available, good working condition, correct size for vehicle 			
Light Beacon 		Tested and working properly 			
Whip Flag 		Available, installed and in good working condition