Title: G21 Truck inspection checklist
Author: RTA

Truck Inspected: | | Inspection Report No: | / T
Make and Model: | | Serial No: |
Owner: | | Inspection Location: |
All Trucks must comply with OHS Act and Regulations, Federal and State legislation and relevant Australian Standards in addition to the requirements set out in RTA G22 Annexure G22/J1
RTA G22 Ed 3 / Rev 2- Schedule J1 | Truck Inspection Findings against Schedule J1 Requirements | N/C / M
J1.1- Registration – Full (J1.1:J1.6.h) | |
| Registration Label in visible location (J1.1) | |
| Windscreen Wipers | |
| | Brake Lights | |
| | Turn Signals | |
| | Head and Tail Lights | |
| | Reflectors | |
| | Rear Marker Plates | |
| | Horn | |
| | Rear Vision Mirrors | |
J1.2 - Safety Standards | Neutral Start (J1.2.1:J1.6.a) | |
| | Brakes (J1.2.2:J1.6.a) | |
| | Brake Air Systems (J1.2.2:J1.6.a) | |
| | Seat Belts (J1.2.3:J1.6.a) | |
| | Reverse Alarm (J1.2.4:J1.6.a) | |
| | Compulsory Signs (J1.2.5) | |
| | Amber Beacon (J1.2.6) | |
J1.3 - Mechanical Requirements | Leaks (J1.3.1) | |
| | Engine (J1.3.2) | |
| | Cooling System (J1.3.3) | |
| | Exhaust System (J1.3.4) | |
| | Exhaust Smoke (J1.3.5:J1.6.g) | |
| | Transmission and Final Drive (J1.3.6) | |
| | Hydraulics (J1.3.7) | |

J1.4 - Cab/Chassis 
Requirements

Chassis (J1.4:J1.6.f)

| | Cabin (J1.4.1) | |
| | Windows (J1.4.2) | |
| | Suspension (J1.4.3:J1.6.e) | |
| | Steering (J1.4.3:J1.6.e) | |
| | Tyres(J1.4.3:J1.6.e) | |
J1.5 - Miscellaneous Requirements | Controls and Switches (J1.5.1) | |
| | Seats (J1.5.2) | |
| | Work Attachments/Tools (J1.5.3) | |
| | Fifth Wheel (Turntable) (J1.5.4) | |
| | Electrical System (J1.5.5) | |
| | Truck Security (J1.5.6) | |
| | Tarping (J1.5.1) | |
| | Truck Body (J1.5.8) | |
| | Tow Bar (J1.5.9) | |
| | Daily Inspection Reports (J1.5.10) | |
Any other condition which could impair the safe operation of the Truck (J1.6.i):
Truck Report By: | | Signature: | | Date: |

Updated by Pentagon Management Pty Ltd, 17 April 2007        Legend:    N/C = Noncompliance with requirements (J1.6)      M = Noncompliance that requires immediate remedial action (All non J1.6)